#!/bin/sh

set -x

speedtest --accept-license --accept-gdpr
mmcli -m 0 --signal-get
mmcli -m 0 --command AT+CPSI?
qmicli --device=/dev/cdc-wdm0 --device-open-proxy --nas-get-signal-strength
qmicli --device=/dev/cdc-wdm0 --device-open-proxy --nas-get-signal-info
qmicli --device=/dev/cdc-wdm0 --device-open-proxy --nas-get-tx-rx-info=lte
qmicli --device=/dev/cdc-wdm0 --device-open-proxy --nas-get-tx-rx-info=5gnr
qmicli --device=/dev/cdc-wdm0 --device-open-proxy --nas-get-home-network
qmicli --device=/dev/cdc-wdm0 --device-open-proxy --nas-get-serving-system
qmicli --device=/dev/cdc-wdm0 --device-open-proxy --nas-get-system-info 
qmicli  --device=/dev/cdc-wdm0 --device-open-proxy --nas-get-technology-preference
qmicli  --device=/dev/cdc-wdm0 --device-open-proxy  --nas-get-system-selection-preference
qmicli  --device=/dev/cdc-wdm0 --device-open-proxy --nas-get-cell-location-info
qmicli  --device=/dev/cdc-wdm0 --device-open-proxy  --nas-get-operator-name
qmicli  --device=/dev/cdc-wdm0 --device-open-proxy  --nas-get-lte-cphy-ca-info
qmicli  --device=/dev/cdc-wdm0 --device-open-proxy  --nas-get-rf-band-info
