#!/bin/bash

cat >> /etc/hosts <<EOF
${JITSI_PROSODY_HOST} jitsi.deuxfleurs.fr conference.jitsi.deuxfleurs.fr jitsi-videobridge.jitsi.deuxfleurs.fr focus.jitsi.deuxfleurs.fr auth.jitsi.deuxfleurs.fr
127.0.0.1 `hostname`
EOF

mkdir -p /root/.sip-communicator

cat > /root/.sip-communicator/sip-communicator.properties <<EOF
# Enable broadcasting stats/presence in a MUC
org.jitsi.videobridge.ENABLE_STATISTICS=true
org.jitsi.videobridge.STATISTICS_TRANSPORT=muc

# Connect to the first XMPP server
org.jitsi.videobridge.xmpp.user.shard.HOSTNAME=jitsi.deuxfleurs.fr
org.jitsi.videobridge.xmpp.user.shard.DOMAIN=auth.jitsi.deuxfleurs.fr
org.jitsi.videobridge.xmpp.user.shard.USERNAME=jvb
org.jitsi.videobridge.xmpp.user.shard.PASSWORD=${JITSI_SECRET_VIDEOBRIDGE}
org.jitsi.videobridge.xmpp.user.shard.MUC_JIDS=JvbBrewery@internal.auth.jitsi.deuxfleurs.fr
org.jitsi.videobridge.xmpp.user.shard.MUC=JvbBrewery@internal.auth.jitsi.deuxfleurs.fr
org.jitsi.videobridge.xmpp.user.shard.MUC_NICKNAME=singleton
org.jitsi.videobridge.xmpp.user.shard.DISABLE_CERTIFICATE_VERIFICATION=true

# Do we need it? @FIXME
org.jitsi.impl.neomedia.transform.srtp.SRTPCryptoContext.checkReplay=false

# NAT things, two times just in case...
org.ice4j.ice.harvest.TCP_HARVESTER_PORT=${JITSI_VIDEO_TCP}
org.ice4j.ice.harvest.NAT_HARVESTER_LOCAL_ADDRESS=${JITSI_NAT_LOCAL_IP}
org.ice4j.ice.harvest.NAT_HARVESTER_PUBLIC_ADDRESS=${JITSI_NAT_PUBLIC_IP}
org.jitsi.videobridge.TCP_HARVESTER_PORT=${JITSI_VIDEO_TCP}
org.jitsi.videobridge.NAT_HARVESTER_LOCAL_ADDRESS=${JITSI_NAT_LOCAL_IP}
org.jitsi.videobridge.NAT_HARVESTER_PUBLIC_ADDRESS=${JITSI_NAT_PUBLIC_IP}
org.jitsi.videobridge.DISABLE_TCP_HARVESTER=false
EOF

[ -v JITSI_DEBUG ] && cat >> /root/.sip-communicator/sip-communicator.properties <<EOF
net.java.sip.communicator.packetlogging.PACKET_LOGGING_ENABLED=true
net.java.sip.communicator.packetlogging.PACKET_LOGGING_ARBITRARY_ENABLED=true
net.java.sip.communicator.packetlogging.PACKET_LOGGING_SIP_ENABLED=true
net.java.sip.communicator.packetlogging.PACKET_LOGGING_JABBER_ENABLED=true
net.java.sip.communicator.packetlogging.PACKET_LOGGING_RTP_ENABLED=true
net.java.sip.communicator.packetlogging.PACKET_LOGGING_ICE4j_ENABLED=true
net.java.sip.communicator.packetlogging.PACKET_LOGGING_FILE_COUNT=1
net.java.sip.communicator.packetlogging.PACKET_LOGGING_FILE_SIZE=-1
EOF

/srv/jvb/jvb.sh \
  --host=${JITSI_PROSODY_HOST} \
  --domain=jitsi.deuxfleurs.fr \
  --port=5347 \
  --secret=${JITSI_SECRET_VIDEOBRIDGE} \
  --apis=xmpp,rest
